**Annexure-IV**



**Commercial Terms and Conditions for Booster Fan**

1. **Performance Guarantee parameters & penalty of the System: R-1**

|  |  |  |
| --- | --- | --- |
| **PG Parameter** | **Guaranteed Value** | **\*L.D. Clause** |
| Capacity& Head shall be guaranteed WITHOUT ANY NEGATIVE TOLERANCE and NO POSITIVE TOLERANCE on POWER Consumed at motor shaft is accepted. | Vendor to indicate these values & provide guarantee for the for the same. | 0.75% of contract value for each kW additional power consumed at BMCR over Guaranteed value subject to a limit of 10% of contract value.  Beyond that the performance to be rectified within 12 months of conducting PG test. |
| M.O.C of various parts of Fan offered | Vendor to stand Guarantee for M.O.C of fan for the duty conditions for a period of 10 years (min.) | Any damage to the parts within that period shall be replaced by the Vendor. |
|  |  |  |

**Vendor shall provide warranty of the total Fan system till the PG test of entire FGD & SAC plant is over.**

**2. Delivery Period:** To be mentioned.

**3. Payment Terms & Other Commercial conditions to be provided by Hindalco.**